View: All

Select your DataMan Reader:

All

DataMan 50

DataMan 60

DataMan 70

DataMan 80

DataMan 150

DataMan 260

DataMan 280

DataMan 290

DataMan 300

DataMan 360

DataMan 370

DataMan 380

DataMan 390

DataMan 470

DataMan 503

DataMan 580

DataMan 7500

DataMan 8050

DataMan 8070

DataMan 8600

DataMan 8700

DataMan 8700 Base Station

Base Station

DataMan MX-1000

DataMan MX-1500

# What is the Xpand ROI settings used for?

You can use this feature to specify the exact region of each part of the image seen by the reader through the FOVE. This can be helpful to disable the ghosting area in the middle of the image where the same code can be detected twice. Reducing the region of interest (ROI) does not necessarily reduce the decoding time or increase the image transfer rate.

The most appropriate settings have been pre-configured for existing Field of View Expanders (FOVEs), but you can fine-tune the settings (Custom setting) by manually adjusting parameters in order to achieve the best results for the particular FOVE in use. Readers, FOVEs, and lens used factor in differently.

NOTE: Some image related properties (eg. image size, filtering) cannot be altered when the device is acquiring or decoding images.

NOTE: Make sure to check if the device you are using is compatible with the FOVE you are trying to calibrate!

Note: DM050, DM060, DM070, DM080, DM150, DM260, DM280, DM290, DM300, DM360, DM370, DM470, DM503