View: All

Select your DataMan Reader:

All

DataMan 50

DataMan 60

DataMan 70

DataMan 80

DataMan 150

DataMan 260

DataMan 280

DataMan 290

DataMan 300

DataMan 360

DataMan 370

DataMan 380

DataMan 390

DataMan 470

DataMan 503

DataMan 580

DataMan 7500

DataMan 8050

DataMan 8070

DataMan 8600

DataMan 8700

DataMan 8700 Base Station

Base Station

DataMan MX-1000

DataMan MX-1500

# What is the Pulse Encoder?

For external trigger modes, you can use an encoder to control the timing of the data string output. Typically encoders are installed on a conveyor belt and as the conveyor belt moves, the encoder shaft will rotate and output electrical pulses to indicate its angular rotation. The amount that the encoder rotates is directly proportional to the distance traveled by the conveyor belt.

Connect your encoder to Input lines 1, 2, or 3. The input line you choose will be exclusively used by the encoder. For any other action, please select another input line.

You can also connect an encoder to a Primary reader in a Multi-Reader Sync group.

Note: DM503