View: All

Select your DataMan Reader:

All

DataMan 50

DataMan 60

DataMan 70

DataMan 80

DataMan 150

DataMan 260

DataMan 280

DataMan 290

DataMan 300

DataMan 360

DataMan 370

DataMan 380

DataMan 390

DataMan 470

DataMan 503

DataMan 580

DataMan 7500

DataMan 8050

DataMan 8070

DataMan 8600

DataMan 8700

DataMan 8700 Base Station

Base Station

DataMan MX-1000

DataMan MX-1500

# How do I use dual Ethernet?

You might use both Ethernet ports of the reader for various reasons, such as:

- Separating out PLC communications for enhanced security. This requires two separate IP addresses, one for image or data saving (Multi-Reader Sync, FTP, PTP), and the other for real-time PLC communication.
- Load balancing by using both Ethernet0 and Ethernet1 ports in separated networks. Use Ethernet0 for real-time critical communications (PTP, industrial protocols, Multi-Reader Sync), and use Ethernet2 for FTP upload.
- Separating image FTP traffic from low-latency tunnel management traffic.

To use dual Ethernet:

1. Enable the second Ethernet port with the Enable Ethernet 1 checkbox.

2. Configure the IP addresses of the ports.

   You can apply the Use Static IP Address option to one or both ports, but only one port can Use DHCP Server.

3. Select which Ethernet port runs PLC communications with the FFP Port dropdown on the Ethernet 0 tab.

Note that on the reader, the physical ports are marked as ENET0 and ENET1.

Note: DM380, DM390, DM580