View: All

Select your DataMan Reader:

All

DataMan 50

DataMan 60

DataMan 70

DataMan 80

DataMan 150

DataMan 260

DataMan 280

DataMan 290

DataMan 300

DataMan 360

DataMan 370

DataMan 380

DataMan 390

DataMan 470

DataMan 503

DataMan 580

DataMan 7500

DataMan 8050

DataMan 8070

DataMan 8600

DataMan 8700

DataMan 8700 Base Station

Base Station

DataMan MX-1000

DataMan MX-1500

# Why isn't the top quadrant of the UltraLight turned on?

In most cases, operators tend to hold the reader at an angle to the surface being read. By disabling the top lighting quadrant, reflections and glare are minimized.

The reader is shipped with default values for each of the four setups, but only the first setup, General Purpose is enabled. The General Purpose setup enables the West, South, and East low-angle lights only. You can modify this setup to enable all of the off-axis light segments.

Note: DM8600, DM8700