View: All

Select your DataMan Reader:

All

DataMan 50

DataMan 60

DataMan 70

DataMan 80

DataMan 150

DataMan 260

DataMan 280

DataMan 290

DataMan 300

DataMan 360

DataMan 370

DataMan 380

DataMan 390

DataMan 470

DataMan 503

DataMan 580

DataMan 7500

DataMan 8050

DataMan 8070

DataMan 8600

DataMan 8700

DataMan 8700 Base Station

Base Station

DataMan MX-1000

DataMan MX-1500

# What can I set with the NoRead Image Mode?

NoRead Image stores only one image per trigger and you can select which one. NoRead Image Period stores every nth bad read image. This is evaluated across trigger modes. For example, if you have Burst trigger mode selected with a length of 5 and set period to 3, the 1st and 4th image of the first, but the 2nd and 5th of the second burst will be stored.

Note: default, DM050, DM060, DM070, DM080, DM150, DM260, DM280, DM290, DM300, DM360, DM370, DM380, DM390, DM380, DM390, DM470, DM503, DM580