View: All

Select your DataMan Reader:

All

DataMan 50

DataMan 60

DataMan 70

DataMan 80

DataMan 150

DataMan 260

DataMan 280

DataMan 290

DataMan 300

DataMan 360

DataMan 370

DataMan 380

DataMan 390

DataMan 470

DataMan 503

DataMan 580

DataMan 7500

DataMan 8050

DataMan 8070

DataMan 8600

DataMan 8700

DataMan 8700 Base Station

Base Station

DataMan MX-1000

DataMan MX-1500

# How do I change the base station's serial port settings?

When you scan the RS-232 Serial configuration code from the Reader Configuration Codes document, the base station is automatically configured to use the same baud rate (and other serial port settings) that the Setup Tool uses.

If you need to connect the base station to a device with a specific baud rate or other serial port settings, scan the appropriate codes from the Reader Configuration Codes document (available through the Windows Start menu or the Setup Tool Help menu). Note that you will need to re-scan the RS-232 Serial or USB Serial code to connect using the Setup Tool.

Note: DM8700Base, DM8000Base