View: All

Select your DataMan Reader:

All

DataMan 50

DataMan 60

DataMan 70

DataMan 80

DataMan 150

DataMan 260

DataMan 280

DataMan 290

DataMan 300

DataMan 360

DataMan 370

DataMan 380

DataMan 390

DataMan 470

DataMan 503

DataMan 580

DataMan 7500

DataMan 8050

DataMan 8070

DataMan 8600

DataMan 8700

DataMan 8700 Base Station

Base Station

DataMan MX-1000

DataMan MX-1500

# What port do I use for a USB Connection?

If you connect the reader or base station using the USB port, make sure to scan the USB-COM/RS-232 configuration code from the Reader Configuration Codes document. Then click Refresh and select the port that is identified as connected to the reader.

Note: Clicking Refresh sends a query string on all COM ports and across the Ethernet network subnet. A DM7550 and a DM8000 wireless reader must be awake in order to respond to the query. Squeeze the trigger to wake up the reader.

Note: default, DMAE50, DM050, DM070, DM150, DM7500, DM8050, DM8070, DM8600, DM8700, DM8700Base, DM8000Base