View: All

Select your DataMan Reader:

All

DataMan 50

DataMan 60

DataMan 70

DataMan 80

DataMan 150

DataMan 260

DataMan 280

DataMan 290

DataMan 300

DataMan 360

DataMan 370

DataMan 380

DataMan 390

DataMan 470

DataMan 503

DataMan 580

DataMan 7500

DataMan 8050

DataMan 8070

DataMan 8600

DataMan 8700

DataMan 8700 Base Station

Base Station

DataMan MX-1000

DataMan MX-1500

# What is the RS-232 Routing option?

When you connect your base station through RS-232, you can change if data is routed to the base station itself, or if you want to communicate directly with the reader associated with the base station.

When no reader is assigned to the base station, the RS-232 interface is used to configure the base station regardless of what you choose in the Routing option. When the associated reader gets assigned or unassigned, the operation mode of the RS-232 interface changes automatically, after you power-cycle your base station.

Note: DM8700Base, DM8000Base