View: All

Select your DataMan Reader:

All

DataMan 50

DataMan 60

DataMan 70

DataMan 80

DataMan 150

DataMan 260

DataMan 280

DataMan 290

DataMan 300

DataMan 360

DataMan 370

DataMan 380

DataMan 390

DataMan 470

DataMan 503

DataMan 580

DataMan 7500

DataMan 8050

DataMan 8070

DataMan 8600

DataMan 8700

DataMan 8700 Base Station

Base Station

DataMan MX-1000

DataMan MX-1500

# What is the Validation Failure Action used for?

The Validation Failure Action is used to determine what is output from the reader after a validation failure. The user can select from different options:

1. Transmit ‘Validation Failure'- The reader will output the string ‘Validation Failure' after a code fails validation
2. Transmit ‘Validation Failure' + decoded string- The reader will output the string ‘Validation Failure' followed by the complete decoded string
3. Transmit annotated decoded string- The reader will output the decoded string along with information on the error type and error location in the string
4. Transmit nothing- The reader will not output any information.
5. Transmit 'Validation Failure' + quoted decoded string- The reader will output the string 'Validation Failure' followed by the quoted part of the decoded string

Note: default, DM050, DMAE50, DM060, DM070, DM150, DM260, DM280, DM290, DM300, DM360, DM370, DM380, DM390, DM470, DM503, DM580, DM8050, DM8070, DM8600, DM8700, MX-1000, MX-1500