View: All

Select your DataMan Reader:

All

DataMan 50

DataMan 60

DataMan 70

DataMan 80

DataMan 150

DataMan 260

DataMan 280

DataMan 290

DataMan 300

DataMan 360

DataMan 370

DataMan 380

DataMan 390

DataMan 470

DataMan 503

DataMan 580

DataMan 7500

DataMan 8050

DataMan 8070

DataMan 8600

DataMan 8700

DataMan 8700 Base Station

Base Station

DataMan MX-1000

DataMan MX-1500

# Which Illumination setting should I select?

Different mark types and mark surfaces can benefit from different lighting sources. The fixed mount lighting supports bright-field illumination for high contrast symbols on non-reflective objects, and dark-field illumination for symbols of low contrast on reflective surfaces. Any combination can be selected if it provides reliable Code Quality grade results.

Be aware that different banks on the fixed mount lighting attachment must be connected to specific output lines on the expanded I/O module, as follows:

- Bright field - diffuse perpendicular (90): I/O line 2, 3

- Dark field - 30 degree all quadrants (30Q): I/O lines 4, 5, 6, 7

- Dark field - 30 degree E-W quadrants (30T): I/O lines 4, 6

- Dark field - 30 degree N-S quadrants (30T): I/O lines 5, 7

Note: DM8600