View: All

Select your DataMan Reader:

All

DataMan 50

DataMan 60

DataMan 70

DataMan 80

DataMan 150

DataMan 260

DataMan 280

DataMan 290

DataMan 300

DataMan 360

DataMan 370

DataMan 380

DataMan 390

DataMan 470

DataMan 503

DataMan 580

DataMan 7500

DataMan 8050

DataMan 8070

DataMan 8600

DataMan 8700

DataMan 8700 Base Station

Base Station

DataMan MX-1000

DataMan MX-1500

# Why can't I send images runtime to an external FTP server at a high frame per second transfer rate?

If you are using settings (Self, Presentation, or External trigger modes) that make it possible to read and transfer images with a 100 frame per second (or higher) rate, the device stores these images into its own image buffer, but you will not be able to send images to an external FTP server.

If you have the Allow Buffer Overwrite option checked, the images will most likely be overwritten. If you have it unchecked, new images will not be buffered until space is available in the buffer again.

Note: DM070, DM080, DM150, DM260, DM280, DM290, DM300, DM360, DM370, DM380, DM390, DM380, DM390, DM470, DM503, DM580