# MASTER-SLAVE.TEST

Transmits the test message from reader to reader as designated by mode. The terminating reader will output the message preceded by the initiating device delimited by a space

## Actions

## Arguments

Name | Type | Range | Meaning
--- | --- | --- | ---
mode |  | [0-2] | 0: Slave to Master 1: Master to Slave 2: Master to Slave to Master
message |  |  |

## Platforms

Fixed-mount readers, except DM80-USB

## Notes

Version: 5.5.0