# IMAGEBUFFER.IMAGE-TYPE

Images to buffer for a result.

Note: Requires the IntImageBuffer feature key to select the "Auto" option. Requires the 3D feature key to select the "3D Image Selection" option.

## Actions

SET/GET Property

## Arguments

Name | Type | Range | Meaning
--- | --- | --- | ---
int |  | [0-7] | 0: All - buffers every acquired image up until the maximum number of images per result or the maximum number of images have been reached. 1: Same as result - buffers every image that matches the IMAGEBUFFER.RECORD-TYPE setting. 2: Auto - when selected, the reader does intelligent image buffering. 3: First - buffers only the first image in the trigger cycle of the specified trigger mode. 4: Last - buffers only the last image in the trigger cycle of the specified trigger mode. 5: First and Last - buffers both the first and the last images in the trigger cycle of the specified trigger mode. 6: 3D Image Selection - when selected, the reader auto selects images by filtering out empty and redundant images. 7: Buffers images only if the distance between the last image is at least equal to the value set by the IMAGEBUFFER.MIN-DISTANCE commands. (Introduced in 6.4.2 SR2)

## Platforms

DM70, DM80, DM150, DM260, DM280, DM290, DM300, DM360, DM370, DM390, DM470, DM503, DM580

## Notes

Version: 5.5.0