View: All

Select your DataMan Reader:

All

DataMan 50

DataMan 60

DataMan 70

DataMan 80

DataMan 150

DataMan 260

DataMan 280

DataMan 290

DataMan 300

DataMan 360

DataMan 370

DataMan 380

DataMan 390

DataMan 470

DataMan 503

DataMan 580

DataMan 7500

DataMan 8050

DataMan 8070

DataMan 8600

DataMan 8700

DataMan 8700 Base Station

Base Station

DataMan MX-1000

DataMan MX-1500

# When should I use the USB Driver Compatibility Mode?

By default, the base station uses a USB driver that can help it recover from an electrostatic discharge (ESD) event. Use USB Driver Compatibility Mode if you require strict conformance to the USB specification or you are using a DataMan base station together with the Cognex SensorView product.

When you change USB driver compatibility mode, the question "The changes made require reboot to take effect. Apply changes and reboot now?" pops up. Click Yes. If, for any reason, you click No, you can still apply the changes. Choose System->Save Settings and then reboot your reader.

Note: DM8700Base, DM8000Base