View: All

Select your DataMan Reader:

All

DataMan 50

DataMan 60

DataMan 70

DataMan 80

DataMan 150

DataMan 260

DataMan 280

DataMan 290

DataMan 300

DataMan 360

DataMan 370

DataMan 380

DataMan 390

DataMan 470

DataMan 503

DataMan 580

DataMan 7500

DataMan 8050

DataMan 8070

DataMan 8600

DataMan 8700

DataMan 8700 Base Station

Base Station

DataMan MX-1000

DataMan MX-1500

# Can I specify characters using hexadecimal or octal ASCII codes?

In the Leading Text and Terminating Text fields, you can specify characters as \nnn where nnn is the octal ASCII code. You can specify characters in hexadecimal by entering \xnn where nn is the hexadecimal ASCII code.

You can also use the following predefined codes:

- \a Alert (ASCII 7)
- \b Backspace(ASCII 8)
- \E Escape (ASCII 27)
- \f form feed (ASCII 12)
- \n line feed (ASCII 10)
- \t horizontal tab (ASCII 9)
- \r carriage return (ASCII 13)
- \v vertical tab (ASCII 11)
- \\ backslash (ASCII 92)

Note: default, DMAE50, DM050, DM060, DM070, DM080, DM150, DM260, DM280, DM290, DM300, DM360, DM370, DM380, DM390, DM470, DM503, DM580, DM7500, DM8050, DM8070, DM8600, DM8700, MX-1000, MX-1500