# Summary of Wireless Buffering Indicators

Condition | Status Indicator: Reader | Status Indicator: Base Station | Sounds
--- | --- | --- | ---
Reader in wireless range of base station | When the reader is awake, blinking BLUE indicates wireless connection with the base. When the reader is offline, there is no indicator. Pull the trigger to wake it up and it will blink BLUE. Good read: GREEN No read: RED | Reader out of the base station and awake: steady BLUE. Reader out of the base station and offline: steady RED. Paired reader in the base station: flashing GREEN. Base station is receiving data or images from reader: steady BLUE. | Good read: 1 beep (default) No read: no beep (default)
Reader base station | Offline: When the reader wakes up out of the wireless range, there is no indicator. Good read: GREEN (default) No read: RED (default) | Reader offline: steady RED. | Long beep when you leave the wireless range. Good read: 2 beeps No read: no beep
Reader out of wireless range of base station, buffer is full | Good read: GREEN and then white. No read: RED (default) | Reader offline: steady RED. | Good read: long beep No read: no beep