# DataMan 8600 Specifications

Specification | DataMan 8600 Reader
--- | ---
Weight | 303 g (without slide-in), 345 g (with tethered slide-in) Wireless: 530 g (18.70 oz) (battery included)
Operating Temperature | 0 ºC — 45 ºC (32 ºF — 113 ºF)
Storage Temperature | DataMan 8600 wireless: -10 ºC — 45 ºC (14 ºF — 113 ºF), DataMan 8600 tethered: -40 ºC — 60 ºC (-40 ºF — 140 ºF)
Maximum Humidity | < 95% (non-condensing)
Environmental | IP65
Symbologies | 1-D barcodes: Codabar, Code 39, Code 128, and Code 93, Interleaved 2 of 5, Pharma, GS1 DataBar, Postal, UPC/EAN/JAN, DataBar 2-D barcodes: Data MatrixTM; QR Code and microQR Code, RSS/CS, PDF 417, MicroPDF 417
Power Supply Requirements | USB: external 5.0 W maximum LPS or NEC class 2 power supply: +5 V - +6 V DC RS232 external 5.0 W max LPS or NEC class 2 power supply +6.0 V 1 A DC (5.0 m RS-232 cable) +6.0 V 1 A DC (2.5 m RS-232 cable) ETH: Class 2 PoE supply IEEE 802.3af (connect only to PoE networks without routing to the outside plant)
Inrush current peak | 5A maximum Duration: approx. 30 μs Electrical charge: 60 μAs at 6 V Maximum capacity: 10 µF Maximum inrush: 50 µC
Battery life for wireless reader (typical use case) | ca. 2900 triggers can be operated within a 10 hour working shift The expected life time of the battery is 5 years.
Ethernet | 10/100 Base-T FULL/HALF DUPLEX, IEEE 802.3
Bluetooth | Bluetooth™ 2.1, 2.4 GHz
Wi-Fi | 802.11 b/g, 2.4 GHz, User Selectable channels 1-11
Protection | Base Station: IP65