# NET-LOCAL.ETHOVERUSB

Enables network communication over USB connection. If you have an active USB connection, you can connect to your device using the IP address of the reader or the base station.

Note: You must reboot the reader or the base station after executing this command.

## Actions

SET/GET Property

## Arguments

Name | Type | Range | Meaning
--- | --- | --- | ---
state | bool | [ON|OFF] | enable/disable

## Platforms

DM8700, DM8700 Base Station USB

## Notes

Version: 6.2.9