# TRAIN.LINESCAN-CAL-FCC

Enables or disables the reader to create flat-field correction data during the linescan alignment process. If successful, the flat-field correction data is applied during the TRAIN.LINESCAN-APPLY command.

## Actions

SET/GET Property

## Arguments

Name | Type | Range | Meaning
--- | --- | --- | ---
state | bool | [ON|OFF] | enable/disable

## Platforms

DM3812 Line Scan

## Notes

Version: 25.4