# INPUT.ACTION

Sets or gets the state for the specified line action.

Note: The given events only take effect on the bidirectional lines if you configured it in the right direction. You can change direction with the IO-LINE.DIRECTION command.

## Actions

SET/GET Property

## Arguments

Name | Type | Range | Meaning
--- | --- | --- | ---
line |  | [0-3] | Input line number
action |  | [0-13] | 0: Train Code 1: Optimize Brightness 2: Set Match String 3: Optimize Focus 4: Read Configuration Code 5: Trigger Off 6: Encoder 7: Allow Buffered No-Read Images 8: Clear Outputs 9: Tune (DM300 only) 10: Encoder direction 11: Trigger on 12: Speed detect A 13: Speed detect B
state |  | [ON|OFF] | ON: execute action when line is triggered OFF: no action

## Platforms

Fixed-mount readers

## Notes

Version: 4.0.0