# CAMERA.LINESCAN-OVERLAP-FRACTION

Sets or gets the fraction of the image that is to be used as overlap between acquisitions. The fraction is 1/n, where n is the value of this argument. A value of 2 means that 1/2 region of the image is overlapping. A value of 10 means that 1/10 region of the image is overlapping.

## Actions

SET/GET Property

## Arguments

Name | Type | Range | Meaning
--- | --- | --- | ---
fraction | int | [2-10] | Denominator in the fraction of overlap. The default value is 3.

## Platforms

DM3812 Line Scan

## Notes

Version: 25.4