# TRUCHECK.CALIBRATE-CUSTOM-ON

Begins the calibration process, using any symbol as a calibration target. In order to calibrate successfully, RMax, RMin, and X-Dimension must match the symbol that is read after the calibration process is started.

## Actions

Command

## Arguments

Name | Type | Range | Meaning
--- | --- | --- | ---
RMax |  | [0.1-100.0] | The RMax value of the calibration target.
RMin |  | [0.1-100.0] | The RMSin value of the calibration target.
XDimension |  | [0.1-100.0] | The X-Dimension of the calibration target.

## Platforms

DM475V, DM8072V

## Notes

Version: 6.1.10