View: All

Select your DataMan Reader:

All

DataMan 50

DataMan 60

DataMan 70

DataMan 150

DataMan 260

DataMan 280

DataMan 300

DataMan 360

DataMan 370

DataMan 470

DataMan 503

DataMan 7500

DataMan 8050

DataMan 8070

DataMan 8600

DataMan 8700

DataMan 8700 Base Station

Base Station

DataMan MX-1000

DataMan MX-1500

# How do I set a delay in the code output?

To set a pause in the code output, the sequence \Pause<time>; can be added to the text fields in the Data Formatting pane.

<time> contains a value in milliseconds, for example, to wait 4 seconds, the sequence is \Pause4000;.

This feature can be used with USB HID or RS232. For RS232, the feature needs to be enable using the DMCC command COM.RS232-ENABLE-PAUSE. For USB HID it is enabled by default.

Note: DM050,DM060,DM070,DM150,DM260,DM300,DM360, DM370,DM280, DM470, DM503,DM8050,DM8070,DM8600,DM8700,MX-1000,MX-1500