View: All

Select your DataMan Reader:

All

DataMan 50

DataMan 60

DataMan 70

DataMan 150

DataMan 260

DataMan 280

DataMan 300

DataMan 360

DataMan 370

DataMan 470

DataMan 503

DataMan 7500

DataMan 8050

DataMan 8070

DataMan 8600

DataMan 8700

DataMan 8700 Base Station

Base Station

DataMan MX-1000

DataMan MX-1500

# Which Light and Imager Settings does the reader use?

You can configure four different read setups. When you attempt to read a code, the reader uses each enabled setup in turn to try to read the code. To enable a setup, click that setup's light at Read Setups or select the setup at the Read Setups pane. Enabled setups are marked with a green light.

When you start a new scan, the reader always starts with the most recently used setup, if multiple setups are enabled. The reader switches the setup based on the number of decode tries, that is, in the default setting the reader will go to the next setup after 2 or 3 unsuccessful decodes. Change the number of decode tries by selecting the Trigger Setup pane under the System Settings group in the tree view.

Note: DM8600,DM8700