View: All

Select your DataMan Reader:

All

DataMan 50

DataMan 60

DataMan 70

DataMan 150

DataMan 260

DataMan 280

DataMan 300

DataMan 360

DataMan 370

DataMan 470

DataMan 503

DataMan 7500

DataMan 8050

DataMan 8070

DataMan 8600

DataMan 8700

DataMan 8700 Base Station

Base Station

DataMan MX-1000

DataMan MX-1500

# Interval Assistant

In the case of Burst, Self and Continuous modes the Interval Assistant can help you make further settings. You can select three ways to calculate the necessary data. In the top right corner select the units (standard or metric) you wish to calculate in.

Click Field of View to calculate the longest possible interval time by measuring the physical field of view and giving the maximum line speed and the size of the longest code.

Click Lens / Distance to Code if you want to give the distance of the code from the lens. Give the focal length from the drop-down and select the direction in which the code is travelling. Here you also need to give the maximum line speed and the size of the longest code.

Click Code Element Size to calculate with the size of the most narrow code element. Enable Test Mode to read your code. You also need to give the direction your code is travelling in, the maximum line speed and the size of the longest code.

At the bottom of the Assistant you get the recommended maximum interval time.

Note: DMAE50,DM050,DM060,DM070,DM150,DM260,DM300,DM360, DM370,DM280, DM470, DM503,MX-1000,MX-1500