View: All

Select your DataMan Reader:

All

DataMan 50

DataMan 60

DataMan 70

DataMan 150

DataMan 260

DataMan 280

DataMan 300

DataMan 360

DataMan 370

DataMan 470

DataMan 503

DataMan 7500

DataMan 8050

DataMan 8070

DataMan 8600

DataMan 8700

DataMan 8700 Base Station

Base Station

DataMan MX-1000

DataMan MX-1500

# What can I change under TUNE button settings?

You can set what input the device uses when the Tune button is pressed on it. By default, the Extended Read Attempts button of the DataMan 8600 is used for Tuning Optimization. Tuning Optimization automatically picks the best Read Setup for the current decode and sets it as an unseen Read Setup 4 in the DataMan Setup Tool, locking in Symbology, Exposure, Lighting Settings, Focus, etc as the other Read Setups are disabled. This provides snappier reading for use cases where the same type of code is read repeatedly.

To execute Tuning Optimization, press and hold the Extended Read Attempts button until a yellow/green light flashes, then let go of the button. The lights continue to flash until a code is read. When the trigger is pressed to read a code, the lights cycle, performing a burst trigger through the enabled Read Setups, then the flashing stops. A beep and solid green light signifies that tuning is over and the reader is optimized. You can undo tuning by holding the Extended Read Attempts button again until the indicator turns red.

Alternative reading options that are utilized by the Extended Read Attempts button can also be selected:

- Train Match String: After arming the device (by holding the Extended Read Attempts button) with the optical button, the next trigger sets the read code as a Match String (feature key required for Match Strings to be available).

- Enable verifier: After arming the device (by holding the Extended Read Attempts button), triggering enables verification on on the read code (feature key required for verification to be available).

To disable the Extended Read Attempts button, use Disable Reader Button here.

Note: DM8600,DM8700