View: All

Select your DataMan Reader:

All

DataMan 50

DataMan 60

DataMan 70

DataMan 150

DataMan 260

DataMan 280

DataMan 300

DataMan 360

DataMan 370

DataMan 470

DataMan 503

DataMan 7500

DataMan 8050

DataMan 8070

DataMan 8600

DataMan 8700

DataMan 8700 Base Station

Base Station

DataMan MX-1000

DataMan MX-1500

# What can I set with the Good Read Image Mode?

Good Read Image stores all buffered good read images unless you set a limit rate.

You can limit the number of good read images that are buffered by choosing Rate limited. Set the read image rate (the number of images buffered and the frequency of this count) and the rate burst, which is the peak rate per the set time.

Note: default,DM260,DM300,DM360, DM370,DM280, DM470, DM503,DM8050,DM8070,DM8600,DM8700