View: All

Select your DataMan Reader:

All

DataMan 50

DataMan 60

DataMan 70

DataMan 150

DataMan 260

DataMan 300

DataMan 360

DataMan 370

DataMan 470

DataMan 503

DataMan 7500

DataMan 8050

DataMan 8070

DataMan 8600

DataMan 8700

DataMan 8700 Base Station

Base Station

DataMan MX-1000

DataMan MX-1500

# What is Buffering Mode?

Single buffering mode allows you to start reading codes even before the wireless connection is fully established. This means that your first read will be a good read even if the reader is still offline. Bad reads are discarded.

In Multiple mode, the reader buffers many good reads up to 1 MB. Bad reads are discarded.

Note: DM8050,DM8070,DM8600,DM8700,MX-1000,MX-1500