View: All

Select your DataMan Reader:

All

DataMan 50

DataMan 60

DataMan 70

DataMan 150

DataMan 260

DataMan 300

DataMan 360

DataMan 370

DataMan 470

DataMan 503

DataMan 7500

DataMan 8050

DataMan 8070

DataMan 8600

DataMan 8700

DataMan 8700 Base Station

Base Station

DataMan MX-1000

DataMan MX-1500

# What does the reader transmit when no code is read?

Normally, no data is transmitted by the reader if a code cannot be read. If you want to know that the reason why you do not see any output is because no data was read, you can specify a specific string up to 32 characters long by using the NoRead Output String in the Basic pane.

Note: default,DMAE50,DM050,DM060,DM070,DM150,DM260,DM300,DM360, DM370, DM470, DM503,MX-1000,MX-1500