View: All

Select your DataMan Reader:

All

DataMan 50

DataMan 60

DataMan 70

DataMan 150

DataMan 260

DataMan 300

DataMan 360

DataMan 370

DataMan 470

DataMan 503

DataMan 7500

DataMan 8050

DataMan 8070

DataMan 8600

DataMan 8700

DataMan 8700 Base Station

Base Station

DataMan MX-1000

DataMan MX-1500

# What are Buffered Image Settings?

Buffered Image Settings control how the reader buffers the images it acquires in response to acquisition triggers as well as the live images taken from any reader. Changing these settings does not affect the performance of the reader, and only affects the image quality and transfer rate between the reader and the Setup Tool.

- size: By default, the Setup Tool displays a quarter of all pixels of each acquired image, or a fraction of each image during a live display. Choosing between image sizes allows the reader to perform a sub-sampling of each image, which can dramatically improve the image transfer speed from the reader to the Setup Tool at the cost of some precise image details.

- format: By default, the reader stores each acquired image in a .jpeg format, which requires less memory and can be transferred from the reader to the Setup Tool faster than a .bmp format image.

- quality: Available only if you are using the .jpeg image format, this slider adjusts internal parameters that allow the reader to perform a smoothing operation on the acquired image which can reduce or enhance the transfer speed from the reader to the Setup Tool.

Note: default,DM050,DM060,DM070,DM150,DM260,DM300,DM360, DM370, DM470, DM503