View: All

Select your DataMan Reader:

All

DataMan 50

DataMan 60

DataMan 70

DataMan 150

DataMan 260

DataMan 300

DataMan 360

DataMan 370

DataMan 470

DataMan 503

DataMan 7500

DataMan 8050

DataMan 8070

DataMan 8600

DataMan 8700

DataMan 8700 Base Station

Base Station

DataMan MX-1000

DataMan MX-1500

# How do I establish a TCP/IP connection?

The reader allows TCP connections to port 23, which is the default TCP port for Telnet applications. If you use a Telnet client, the only parameter you will have to provide is the reader's IP address. If you are using another application or SDK to connect, make sure that it uses the same TCP port setting as your reader does. The TCP port can be changed on the Telnet pane. The reader will automatically send code output over this connection. You are able to transmit DataMan Control Commands (DMCC) over this connection as well.

When you change the Telnet port, the question "The changes made require reboot to take effect. Apply changes and reboot now?" pops up. Click Yes. If, for any reason, you click No, you can still apply the changes. Choose System->Save Settings and reboot your reader.

Note: DMAE50,DM060,DM070,DM260,DM300,DM360, DM370, DM470, DM503,DM8050,DM8070,DM8600,DM8700,MX-1000,MX-1500