View: All

Select your DataMan Reader:

All

DataMan 50

DataMan 60

DataMan 70

DataMan 150

DataMan 260

DataMan 300

DataMan 360

DataMan 370

DataMan 470

DataMan 503

DataMan 7500

DataMan 8050

DataMan 8070

DataMan 8600

DataMan 8700

DataMan 8700 Base Station

Base Station

DataMan MX-1000

DataMan MX-1500

# What data does Code Quality Overview collect and display?

Code Quality Overview can display code quality grades and metrics in a real-time graph, depending on the setting in the top left under Settings > Plotted Value. Select the metric or grade you want to monitor on the device. Only the code quality standard that is set on the monitored device is available under Plotted Value (so an empty dropbox means that no standard is enabled on the device). You can collect data for another standard by changing the enabled code quality standard on the target device.

In case of multicode, there may be multiple code quality standards set on the device. In this case, the graph displays two data lines (and their average is displayed above).

NOTE: Because RTM Lean uses a 1 minute minimum interval, grades can have an intermediate value.

The Last [time interval] buttons on the top row are clickable, and the active is outlined orange. You can use the buttons to set the interval that Code Quality Overview uses. The average plotted value is displayed here.

You can set up a warning line to appear on the graphs under Configuration > Display Settings. Ticking the box makes the warning line to display on each graph. Chart Type determines what kind of line is displayed, while ReadRate Reference Line Value (%) is the percentage where the line is drawn on the graphs.

Note: DM060,DM260,DM300,DM360, ,DM503, DM370, DM470, RTM_Lean