# PROFINET.ENABLED

Enabled or disabled PROFINET communications.

## Actions

SET/GET Property

## Arguments

Name | Type | Range | Meaning
--- | --- | --- | ---
state | bool |  |

## Platforms

Ethernet readers. The DM8000 wireless readers also support this protocol if the base station is connected through Ethernet. In the case of a Bluetooth connection, the command has to be sent to the base station, not to the reader.

## Notes

Version: 3.0.0