# PCM.METRIC-PARM-REPORT

Include the metric grading result for selected quality standard and metric in the report if enabled. Only available if not use for overall calculation (e.g. ISO-IEC 15415 → Modulation → Show in Report = ON) Not all metrics are available for each standard: AIM-DPM (0, 1, 2, 3, 4, 5, 6, 8), ISO-IEC 15415 (0, 1, 2, 3, 4, 5, 6, 7), ANSI-ISO-IEC 15416 (0, 4, 8, 9, 22, 23, 24, 25), SemiT10 (1, 4, 12, 13, 14, 15, 16, 17, 18, 19, 20), 1D readability (0, 2, 8, 9, 10, 11), DotCode (0, 1, 2, 3, 6, 8).

## Actions

SET/GET Property

## Arguments

Name | Type | Range | Meaning
--- | --- | --- | ---
type |  | [0-5] | 0: AIM-DPM
type |  | [0-27] | 0: Symbol Contrast
state |  | [ON|OFF] | ON: include in report

## Platforms

Ethernet readers.

## Notes

Version: 5.7.0