# IMAGEBUFFER.NO-READ-IMAGE-PERIOD

Sets or gets the interval to save the image of a bad read. If, for example, you use an interval of 6, the first bad image is saved and the next 5 are not. The default is 1 which saves each bad read image.

## Actions

SET/GET Property

## Arguments

Name | Type | Range | Meaning
--- | --- | --- | ---
interval | int | [1-1024] |

## Platforms

DM50, DM60, DM70, DM503, and DM300, DM360, DM370, DM470, only in Single, Burst, Self and Continuous modes.

## Notes

Version: 4.0.0