# OUTPUT.USER-CONFIGURE

Sets the beeper tone, number of beeps, LED color, and vibration state for USER_EVENT_1 or USER_EVENT_2. Note: The DM8050 will ignore the vibration state, but the parameter is still required.

## Actions

SET/GET Property

## Arguments

Name | Type | Range | Meaning
--- | --- | --- | ---
event number |  | [1,2] | 1: USER_EVENT_1
beep tone |  | [0-2] | [0]: Low
beep number |  | [0-3] | Number of beeps
LED color |  | [0-7] | [0]: Off
vibration | bool |  | ON: The reader vibrates on the given user event.

## Platforms

DM8050, DM8600, MX1000.

## Notes

Version: 5.3.0