View: All

Select your DataMan Reader:

All

DataMan 50

DataMan 60

DataMan 70

DataMan 150

DataMan 260

DataMan 300

DataMan 360

DataMan 370

DataMan 470

DataMan 503

DataMan 7500

DataMan 8050

DataMan 8070

DataMan 8600

DataMan 8700

DataMan 8700 Base Station

Base Station

DataMan MX-1000

DataMan MX-1500

# What are the different settings for EAN.UCC Composite Properties?

- Standard (linear and 2D): Consists of a linear component (encoding the item's primary identification) associated with an adjacent 2D Composite Component (encoding supplementary data, such as a batch number or expiration date)

- Linear-only: Consists of only the linear component encoding the item's primary identification.

Note: default,DMAE50,DM050,DM060,DM070,DM150,DM260,DM300,DM360, DM370, DM470, DM503,DM7500,DM8050,DM8070,DM8600,DM8700,MX-1000,MX-1500