View: All

Select your DataMan Reader:

All

DataMan 50

DataMan 60

DataMan 70

DataMan 150

DataMan 260

DataMan 300

DataMan 360

DataMan 370

DataMan 470

DataMan 503

DataMan 7500

DataMan 8050

DataMan 8070

DataMan 8600

DataMan 8700

DataMan 8700 Base Station

Base Station

DataMan MX-1000

DataMan MX-1500

# What is the Allow Buffered NoRead Images option?

When this input is active and connected to, for instance, a package detecting sensor, even though buffering might be applied for all images, the NoRead images will only be buffered when the sensor raises a signal to the particular input. As a result, the reader will only buffer NoRead images when the sensor actually detects a package. This option only works in Continuous trigger mode.

Note: DM050,DM060,DM070,DM150,DM260,DM300,DM360, DM370, DM470, DM503