View: All

Select your DataMan Reader:

All

DataMan 50

DataMan 60

DataMan 70

DataMan 150

DataMan 260

DataMan 300

DataMan 360

DataMan 370

DataMan 470

DataMan 503

DataMan 7500

DataMan 8050

DataMan 8070

DataMan 8600

DataMan 8700

DataMan 8700 Base Station

Base Station

DataMan MX-1000

DataMan MX-1500

# How do I use an external light source?

In the Advanced tab of Optimize Image pane, select External for the illumination type.

To use an external light, connect it to the selected output line as described in the Quick Reference Guide.

- The output line must be wired as a current sink.

- The common output must be logical ground.

- The limit for current is 50 mA @ 24 VDC.

Note: DM300