# KEY.SEND-PHYSICAL-CONTROL-CHARACTERS

When you enable this command, physical keys are used in HID messages for those control characters that have a physical equivalent in the keyboard. For example, you can use [Tab] for 0x09. For those control characters that do not have a physical equivalent, use the KEY.CONTROL-CHARACTERS-MAPPING command to set a key combo for HID messages.

## Actions

SET/GET Property

## Arguments

Name | Type | Range | Meaning
--- | --- | --- | ---
state | bool | [ON|OFF] | enable/disable

## Platforms

DM8700 USB, DM8700 Base Station USB

## Notes

Version: 6.2.7