# COM.USB-HID-NO-OUT-ENDPOINT

When enabled, you can use the SETUP/SET_REPORT method to receive reports from the host. When disabled, you can use the OUT Endpoint for this purpose.

## Actions

SET/GET Property

## Arguments

Name | Type | Range | Meaning
--- | --- | --- | ---
state | bool | [ON|OFF] | enable/disable

## Platforms

DM8700 base station USB, DM8700 wired USB

## Notes

Version: 6.2.7