View: All

Select your DataMan Reader:

All

DataMan 50

DataMan 60

DataMan 70

DataMan 150

DataMan 260

DataMan 300

DataMan 360

DataMan 370

DataMan 470

DataMan 503

DataMan 7500

DataMan 8050

DataMan 8070

DataMan 8600

DataMan 8700

DataMan 8700 Base Station

Base Station

DataMan MX-1000

DataMan MX-1500

# How do I change the output of non-printable ASCII characters to keyboard recognizable equivalents?

Go to the Non-Printing Characters pane under Communication Settings and check Enabled. You can also add non-printable ASCII commands before and after the converted string by enabling Standard Formatting and adding ASCII commands before or after the full string.

Note: default,DMAE50,DM050,DM060,DM070,DM150,DM260,DM300,DM360, DM370, DM470, DM503