View: All

Select your DataMan Reader:

All

DataMan 50

DataMan 60

DataMan 70

DataMan 150

DataMan 260

DataMan 300

DataMan 360

DataMan 370

DataMan 470

DataMan 503

DataMan 7500

DataMan 8050

DataMan 8070

DataMan 8600

DataMan 8700

DataMan 8700 Base Station

Base Station

DataMan MX-1000

DataMan MX-1500

# What are the different Transfer Modes?

On Request transfer mode transfers images when you click Transfer Now in the Setup Tool or you send the appropriate DMCC. If you choose the FTP - Runtime transfer mode, images are automatically sent to the FTP server as soon as the connection becomes alive.

Note that Transfer Now does not work when out of range of the base station paired with the device (in case of handheld devices), as the buffer is cleared and disabled when out of range.

Note: DM8050,DM8070,DM8600,DM8700,MX-1000,MX-1500