View: All

Select your DataMan Reader:

All

DataMan 50

DataMan 60

DataMan 70

DataMan 150

DataMan 260

DataMan 300

DataMan 360

DataMan 370

DataMan 470

DataMan 503

DataMan 7500

DataMan 8050

DataMan 8070

DataMan 8600

DataMan 8700

DataMan 8700 Base Station

Base Station

DataMan MX-1000

DataMan MX-1500

# How do I generate a Validation Pass event?

If data validation is activated, the Read event only gets signaled if a code was read and validation passed. With Read and NoRead events assigned to two outputs the following logic applies:

1. good read, validation pass: Read output

2. good read, validation failure: no output

3. bad read: Bad Read output

Alternatively, you can assign the Validation Failure event to an output.

Note: DM050,DM060,DM070,DM150,DM260,DM300,DM360, DM370, DM470, DM503