View: All

Select your DataMan Reader:

All

DataMan 50

DataMan 60

DataMan 70

DataMan 150

DataMan 260

DataMan 300

DataMan 360

DataMan 370

DataMan 470

DataMan 503

DataMan 7500

DataMan 8050

DataMan 8070

DataMan 8600

DataMan 8700

DataMan 8700 Base Station

Base Station

DataMan MX-1000

DataMan MX-1500

# What can I set under the 2D Codes tab?

After you set up your device to compute ISO/IEC 15415, AIM-DPM/ISO/IEC TR29158, SEMI T10, or DotCode for 2D Codes (under the General tab in the Code Quality pane), this tab allows you to manage aspects of that type of code grading.

In the Minimum Pass Grade for Overall Result drop down box you can specify what minimum grade is accepted as a 'Pass' for the given code quality standard.

By ticking the Custom Threshold checkbox, you can overrule and customize the custom threshold settings originally defined in the given code quality standard. Note that if you uncheck and re-check the checkbox, the threshold values are reset to their default. These options provide a list of metrics for the standard, and each of these metrics have the following settings:

- Threshold can be set for the grades A, B, C and D. If a metric value exceeds this threshold, the respective grade is assigned. Grade F is assigned if the value does not reach threshold of grade D. Note that some metrics (eg. SEMI 10) do not have thresholds, this is according to the ISO standards (for details, see http://www.iso.org for the respective ISO standard documentation).

- Use for overall calculation: if ticked, this metrics is used for the calculation of the overall grade. Note that SEMI T10 metrics do not have this option.

- Include in report: if ticked, this metric is included in the code quality report available directly from the reader via FTP transfer or generated from Setup Tool via report logging, and in the result string that can be enabled in the tab Result String.

Note that due to their nature not all metrics have all options available (for example if the ISO standard does not assign a grade to the metric).

Note: MicroQR is not supported for 2D code quality grading.

Note: DM050,DM060,DM070,DM150,DM260,DM300,DM360, DM370, DM470, DM503,MX-1000,MX-1500