View: All

Select your DataMan Reader:

All

DataMan 50

DataMan 60

DataMan 70

DataMan 150

DataMan 260

DataMan 300

DataMan 360

DataMan 370

DataMan 470

DataMan 503

DataMan 7500

DataMan 8050

DataMan 8070

DataMan 8600

DataMan 8700

DataMan 8700 Base Station

Base Station

DataMan MX-1000

DataMan MX-1500

# What is the NoRead Image Period?

The NoRead Image Period is the rate at which NoRead images are buffered. If the value is set to 1, then all NoRead images are buffered. If you set the value to an integer N, where N is greater than 1, then only every Nth image is buffered.

Setting a NoRead Image Period value greater than 1 allows you to reduce the number of NoRead images that are buffered.

The NoRead Image Period value also affects image buffering if What Results to Buffer is set to read, because when read images are buffered, all of the images associated with a single read trigger are marked as read, so previously acquired NoRead images may be buffered as well. Setting the NoRead Image Period value can reduce the number of these images that are buffered.

Note: default,DM050,DM060,DM070,DM150,DM260,DM300,DM360, DM370, DM470, DM503