# Action Overview

Command | Supported Platforms
--- | ---
BACKUP.EXPORT | ALL
BEEP | ALL
BEEP.GLOBAL-ENABLE | DM8050, DM8600
COM.BUFFER-RESET | DM8050, DM8600 and MX-1000.
COM.BUFFER-START-SEND | DM8050, DM8600 and MX-1000.
CONFIG-BACKUP.ENABLE | Ethernet readers. DM8000 wireless readers also support FTP if the base station is connected through Ethernet.
CONFIG-BACKUP.IP-ADDRESS | Ethernet readers. DM8000 wireless readers also support FTP if the base station is connected through Ethernet.
CONFIG-BACKUP.PASSWORD | Ethernet readers. DM8000 wireless readers also support FTP if the base station is connected through Ethernet.
CONFIG-BACKUP.PORT | Ethernet readers. DM8000 wireless readers also support FTP if the base station is connected through Ethernet.
CONFIG-BACKUP.USER-NAME | Ethernet readers. DM8000 wireless readers also support FTP if the base station is connected through Ethernet.
CONFIG.DEFAULT | ALL
CONFIG.EXPORT | ALL
CONFIG.LOAD | ALL
CONFIG.RESTORE | ALL
CONFIG.SAVE | ALL
CONFIG.SEND | ALL
DEVICE-LOG.CLEAR | DM50, DM60, DM70, DM300, DM360, DM503, DM8050, DM8600, MX-1000 and MX-1502.
DEVICE.BACKUP | ALL
DEVICE.DEFAULT | ALL
DEVICE.LOG | DM50, DM60, DM70, DM280, DM300, DM360, DM370, DM470, DM503, DM8050 and DM8600.
DEVICE.RESTORE | ALL
DEVICE.STATS | ALL
DEVICE.TIMEZONE | All
DMCC.RESET | ALL
DMCC.SAVE | ALL
HPIT.AUTOFOCUS-CONTROL-ENABLE | DM370, DM470 with HPIT.
HPIT.DISTANCE-BASED-TRIGGERING-ENABLED | DM370, DM470 with HPIT.
HPIT.EXPANDED-FOCUS-ENABLED | DM370, DM470 with HPIT.
HPIT.EXPANDED-FOCUS-POWER-LIMIT-CDPT | DM370, DM470 with HPIT.
HPIT.EXPANDED-FOCUS-STEPS | DM370, DM470 with HPIT.
HPIT.INDICATOR-ON-TIME | DM370, DM470.
HPIT.OUTPUT-CONFIG-CUSTOM-INDICATOR | DM370, DM470.
HPIT.OUTPUT-CUSTOM-INDICATOR-ENABLE | DM370, DM470 with HPIT.
HPIT.RANGE-DETECTION-BOUNDED-FOCUS-ENABLED | DM370, DM470 with HPIT.
HPIT.RANGE-DETECTION-ENABLED | DM370, DM470 with HPIT.
HPIT.RANGE-DETECTION-MAX-DISTANCE | DM370, DM470 with HPIT.
HPIT.RANGE-DETECTION-MIN-DISTANCE | DM370, DM470 with HPIT.
IMAGE.SEND | ALL
INPUT.STATE | Fixed-mount readers
KEY.PAUSE-TIME | DM8050, DM8600
MIRROR.ANGLE-DIRECT | DM370, DM470 equipped with High Speed Steerable Mirror
MIRROR.ANGLE-POSITION | DM370, DM470 equipped with High Speed Steerable Mirror
MIRROR.MOVE-ENABLED | DM370, DM470 equipped with High Speed Steerable Mirror
MIRROR.POSITIONS | DM370, DM470 equipped with High Speed Steerable Mirror
MOTION-DETECTION.ACTIVE | DM50, DN60, DM70, DM150, DM260, DM280, DM300, DM360, DM370, DM470
MOTION-DETECTION.ENABLE | DM50, DN60, DM70, DM150, DM260, DM280, DM300, DM360, DM370, DM470, DM503.
MOTION-DETECTION.SENSITIVITY | DM50, DM60, DM70, DM150, DM260, DM280, DM300, DM360, DM503.
MOTION-DETECTION.SENSITIVITY | DM370, DM470, DM8700.
OUTPUT.DATAVALID-FAIL | ALL
OUTPUT.GOOD | ALL
OUTPUT.NOREAD | ALL
OUTPUT.USER1 | DM8050, MX-1000, MX-1502, DM300, DM360, DM370, DM470, DM503
OUTPUT.USER2 | DM8050, MX-1000, MX-1502, DM300, DM360, DM370, DM470, DM503
REBOOT | ALL
REBOOT.DELAYED | All
RESULT | ALL
STATISTICS.RESET | ALL
TRAIN.BRIGHT | Fixed mount devices.
TRAIN.CODE | Fixed mount devices.
TRAIN.FOCUS | DM503 and DM300, DM360, DM370, DM470.
TRAIN.MATCH-STRING | Fixed mount devices, DM8050 and DM8600.
TRIGGER | ALL
TRIGGER | ALL
TUNE.CANCEL | DM280, DM300, DM360, DM370, DM470, DM70, DM260, and DM150.
TUNE.START | DM280, DM300, DM360, DM370, DM470, DM70, DM260, and DM150.
TUNE.STATUS | Fixed mount devices.
UNTRAIN.MODEL | Fixed mount readers.
UPTIME | All
WEBHMI.ACTIONS | DM370 and DM470.
WEBHMI.ENABLE | DM370 and DM470
WEBHMI.LANGUAGE | DM370 and DM470
WEBHMI.MATCH-STRING | DM370 and DM470
WEBHMI.SETTINGS | DM370 and DM470