# IMAGEBUFFER.IMAGE-TYPE

Sets "What images to Buffer for a Result". “All” will buffer every acquired image up until the maximum number of images per result or the maximum number of images have been reached. “Same as result” will buffer every image that matches the IMAGEBUFFER.RECORD-TYPE setting. "Auto", when selected, the reader does intelligent image buffering. “First” will buffer only the first image in the trigger cycle of the specified trigger mode. “Last” will buffer only the last image in the trigger cycle of the specified trigger mode. “First and Last” will buffer both the first and the last images in the trigger cycle of the specified trigger mode.

## Actions

SET/GET Property

## Arguments

Name | Type | Range | Meaning
--- | --- | --- | ---
int |  | [0-5] | 0: All 1: Same as result 2: Auto 3: First 4: Last 5: First and Last

## Platforms

DM70, DM150, DM260, DM280, DM300, DM360, DM370, DM470, DM503

## Notes

Version: 5.5.0