# MIRROR.ANGLE-POSITION

Get/set the stored angle values corresponding to the given path position index. For single axis motion, α or β may be expanded to +/- 25.000°.

## Actions

SET/GET Property

## Arguments

Name | Type | Range | Meaning
--- | --- | --- | ---
index | uint8 | [0-63] | SET MIRROR. ANGLE-POSITION 2 10.5 10.5
float | data | [-17° - +17°] | Append/Set an angle value in a given position on angle_a.
float | data | [-17° - +17°] | Append/Set an angle value in a given position on angle_b.

## Platforms

DM370, DM470 equipped with High Speed Steerable Mirror

## Notes

Version: 6.1.10