# IMAGEBUFFER.GOOD-IMAGE-RATE-TIME

Time unit of good read images to be buffered at a rate number specified with IMAGEBUFFER.GOOD-IMAGE-RATE-TIME.

## Actions

SET/GET Property

## Arguments

Name | Type | Range | Meaning
--- | --- | --- | ---
type | enum | [0-3] | 0: seconds 1: minutes 2: hours 3: days

## Platforms

DM280, DM300, DM360, DM370, DM470, DM503, DM8050 and DM8600.

## Notes

Version: 5.2.0